NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor channels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [315 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

KCRC125 Commercial Range Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Box Channel

• Type: KCRC125

• Length: 1000mm / 2000mm / 3000mm

• Loading class to BS EN 1433: A15

• Fall: No Fall

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Channel profile: Standard

• Flange: Flange connection at channel joint and neoprene gasket

• Gully: Central Gully 110mm Spigot / End Gully 110mm Spigot

• Grating: Kent Customised /Kent Diamond Perforated /Kent Interceptor /Kent Pedestrian Heelmesh /Kent Square Perforated /Kent Tetra /Kent Wedge Heelmesh

Product Specification:

KCRC125 Commercial Range Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Box Channel

• Type: KCRC125

• Length: 3000mm

• Loading class to BS EN 1433: A15

• Fall: No Fall

• Material: 1.4301 (304) stainless steel

• Channel profile: Standard

• Flange: Flange connection at channel joint and neoprene gasket

• Gully: Central Gully 110mm Spigot

• Grating: Square Perforated Grating apped