NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/302 Floor channels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-Drainage-ChannelsKSBC150BoxChannel)

* [310 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-Drainage-ChannelsKSBC150BoxChannel)

Product Specification:

KSCC27 Hex Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent SuperClean Channel

• Type: KSCC27 / KSC50 / KSCC70

• Length:

• Loading class to BS EN 1433: A15 /B125 /C250 /D400

• Fall: Fall 150’ to ‘Fall 1:150 (0.67%) /Fall 1:50 (2%) /Fall 1:100 (1%)

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Channel profile: Box section reinforcement /Double box section reinforcement /Round bottom /Safety edge /Solid bar reinforcement /Standard /'V' bottom

• Flange: Flange connection at channel joint and neoprene gasket /Flange flush with channel joint

• Gully: Central Gully KV215/110 /End Gully KV215/110

• Grating:

Suggested Specification:

KSCC27 Hex Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent SuperClean Channel

• Type: KSCC27

• Length: 3000mm

• Loading class to BS EN 1433: B125

• Fall: Fall 1:150 (0.67%)

• Material: 1.4301 (304) stainless steel

• Channel profile: Standard

• Flange: Flange connection at channel joint and neoprene gasket

• Gully: End Gully KV215/110

• Grating (on Gully): Kent Ladder Grating KLG150