NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/334 Stainless steel rodding eyes

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKR161RoddingEye)

* [390 RODDING EYES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKR161RoddingEye)

Product Specification:

KENT KRE170TP (SQ) - Commercial Rodding Eye (High Footfall) • Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: KENT KRE170TP (SQ) - Commercial Rodding Eye (High Footfall) • Material: Stainless steel, grade 304 (1.4301) /Stainless steel, grade 316 (1.4401)

• Accessories/ Other requirements: Not required /Damp proof membrane /Holding flange /Slip-resistant cover plate

Suggested Specification:

KENT KRE170TP (SQ) - Commercial Rodding Eye (High Footfall) • Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: KENT KRE170TP (SQ) - Commercial Rodding Eye (High Footfall) • Material: Stainless steel, grade 316 (1.4401)

• Accessories/ Other requirements: Not required