NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/products/buildings-in-the-landscape/B91.aspx)

* [420 WAITING SHELTER](https://www.ribaproductselector.com/products/waiting-shelter/B91_420.aspx)

Product Specification:

Kent Airport Shelter KAS/5

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Airport Shelter KAS/5

• Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

• Glass: 20mm toughened and laminated

• Size :

* Width : 2341 mm /Special order
* Length: 7750 mm /Special order
* Height: 2734 mm /Special order

• Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened

• Installation Type: Buried flange /Cast-in /Visible flange

• Accessories/ Other requirements: Integrated seat / floor mounted bump rail / lighting / advertising panels

Suggested Specification:

Kent Airport Shelter KAS/5

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Airport Shelter KAS/5

• Material: 1.4404 (316L) stainless steel

• Glass: 20mm toughened and laminated

• Size :

* Width : 2341 mm
* Length: 7750 mm
* Height: 2734 mm

• Finish: Bright satin

• Installation Type: Buried flange

• Accessories/ Other requirements: Integrated seat / floor mounted bump rail / lighting /