NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:



This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

* [340 CYCLE SHELTER](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

Product Specification:

Kent Carrickmines Waiting Shelter KCWS660

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Carrickmines Waiting Shelter KCWS660

 • Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

 • Size :

* Width : 1800 mm /Special order
* Length: 6600 mm /Special order
* Height: 2475 mm /Special order

 • Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened

 • Glass: 12mm toughened and laminated

 • Installation Type: Buried flange /Cast-in /Visible flange / 2 stage cast in

 • Accessories/ Other requirements: Integrated seat / floor mounted bump rail / lighting /

Suggested Specification:

Kent Carrickmines Waiting Shelter KCWS660

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Carrickmines Waiting Shelter KCWS660

 • Material: 1.4404 (316L) stainless steel

 • Size :

* Width : 1800 mm
* Length: 6600 mm
* Height: 2475 mm

 • Finish: Bright satin

 • Glass: 12mm toughened and laminated

 • Installation Type: 2 stage cast in

 • Accessories/ Other requirements: Integrated seat / floor mounted bump rail / lighting