NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Access-CoversKentHingedVinylManholeKMHD600VHLA)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Access-CoversKentHingedVinylManholeKMHD600VHLA)

Product Specification:

Kent Hinged Vinyl Manhole

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Hinged Vinyl Manhole

• Type: KMHD-300/300VHLA /KMHD-450/450VHLA /KMHD-600/600VHLA /KMHD-750/750VHLA / KMHD-900/750 VHLA / KMHD-900/900VHLA

• Size: Bespoke /Manufacturer's standard

• Load class: FACTA A /FACTA AA /FACTA AAA /FACTA B /FACTA C /FACTA D

• Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel

• Seal: Single /Double /Triple

• Fire panels: Not required /Required

Suggested Specification:

Kent Hinged Vinyl Manhole

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Hinged Vinyl Manhole

• Type: KMHD-900/900VHLA

• Size: 900mm x 900mm clear opening

• Load class: FACTA AAA

• Material: 1.4404 (316L) stainless steel

• Seal: Double

• Fire panels: Not required