NBS Specification:



This product is associated with the following NBS Create clause:

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

* [305 PROPRIETARY ACCESS AND INSPECTION CHAMBERS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

Product Specification:

Kent Manhole Inspection Liner KMILDC1000

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Manhole Inspection Liner

• Type: KMILDC850-850/4"/6" / KMILDC900-900/4"/6" / KMILDC900-900/6"/8" / KMILDC1000-1000/4"/6" / KMILDC1000-1000/6"/8" / KMILDC1200-1200/4"/6" / KMILDC1200-1200/6"/8"

• Loading to BS EN 1433: B125 /C250 /D400

• Body size: Manufacturers standard / custom

• Inlet:

- Size: 4”-6”; 6”-8”

- Quantity: 1 /2 /3 /As drawing

- Double contained

Suggested Specification:

Kent Manhole Inspection Liner KMILDC1000

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Manhole Inspection Liner

• Type: KMILDC900-900/4"/6"

• Loading to BS EN 1433: B125

• Body size: 900mm x 900mm x 750mm (h)

• Inlet:

- Size: Inlet 1: 4”-6”; inlet 26”-8”

- Quantity: 2

- Double contained