NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/products/trenches-pipeways-and-pits-for-buried-engineering-services/P30.aspx)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-manhole-tops-and-frames/P30_301.aspx)

[P31 Holes, chases, covers and supports for services](https://www.ribaproductselector.com/products/holes-chases-covers-and-supports-for-services/P31.aspx)

* [370 ACCESS COVERS/ GRATINGS FOR](https://www.ribaproductselector.com/products/access-covers-gratings-for/P31_370.aspx)

[R12 Below ground drainage systems](https://www.ribaproductselector.com/products/below-ground-drainage-systems/R12.aspx)

* [471 ACCESS COVERS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-and-frames/R12_471.aspx)

Product Specification:

Kent Multi Chequer manhole KMCHQ-1200/1200

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Multi Chequer manhole KMCHQ-1200/1200

• Type: KMCHQ-1200/600 /KMCHQ-1200/1200 /KMCHQ-1800/600 /KMCHQ-1800/1200 /KMCHQ-1800/1800 /KMCHQ-2400/600 /KMCHQ-2400/1200 /KMCHQ-2400/1800

• Size: Bespoke /Manufacturer's standard

• Load class: BS EN 124 A15 /BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400 /FACTA A /FACTA AA /FACTA AAA /FACTA B /FACTA C /FACTA D

• Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

• Tray depth: 50mm /80 mm /100 mm

• Seal: Required (double sealed) /Not required

• Lettering (lifting corners): Required /Not required

• Safety barrier: Required /Not required

• Safety grid: Required /Not required

Suggested Specification:

Kent Multi Chequer manhole KMCHQ-1200/1200

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Multi Chequer manhole KMCHQ-1200/1200

• Type: KMCHQ-2400/600

• Size: Manufacturer's standard - 2400mm x 600mm clear opening

• Load class: BS EN 124 A15

• Material: 1.4404 (316L) stainless steel

• Tray depth: 100 mm

• Seal: Required (double sealed

• Lettering (lifting corners): Required as per project requirement

• Safety barrier: Required

• Safety grid: Required