NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:



This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/products/buildings-in-the-landscape/B91.aspx)

* [320 BUS SHELTER](https://www.ribaproductselector.com/products/bus-shelter/B91_320.aspx)
* [420 WAITING SHELTER](https://www.ribaproductselector.com/products/waiting-shelter/B91_420.aspx)

Product Specification:

Kent Round Top Shelter KRTS/5

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Round Top Shelter KRTS/5

 • Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel

 • Size :

* Width : 2030 mm /Special order
* Length: 7546 mm /Special order
* Height: 2526 mm /Special order

 • Finish : Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened / Powder-coated, metallic black /Powder-coated, RAL /Other

 • Installation Type: Buried flange /Cast-in /Visible flange / 2 stage cast in

 • Accessories/ Other requirements: Integrated Seating/floor mounted bump rail / lighting / RTPI Sign / Help Point / advertising panels

Suggested Specification:

Kent Round Top Shelter KRTS/5

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Round Top Shelter KRTS/5

 • Material: 1.4404 (316L) stainless steel

 • Size :

* Width : 2030 mm
* Length: 7546 mm
* Height: 2526 mm

 • Finish : Bright peened

 • Installation Type: Buried flange

 • Accessories/ Other requirements: Integrated Seating/floor mounted bump rail / lighting / RTPI Sign / Help Point / advertising panels