NBS Specification:



This product is associated with the following NBS Create clause:

45-75-95/465 Wall protection panels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

[170 PROPRIETARY](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

Product Specification:

Kent Stainless Double Sided Kerbing

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Stainless Double Sided Kerbing

• Type: KDSK290 /KDSK630

• Material:

- Type: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

- Thickness: 2 mm /3 mm

- Finish: 320 grit polished and electropolished /Bead blasted /Bead blasted and electropolished /Electropolished /Satin, 320 grit polished /Powder coated

• Fixing: Buried flange /Cast in /Flange /Hidden flange

• Cowl: Required /Not required