NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:



This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentTripleSealWaterTight)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentTripleSealWaterTight)

Product Specification:

Kent Triple Seal Water Tight

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Triple Seal Water Tight Manhole

 • Type: KMHT(W)-300/300 /KMHT(W)-450/450 /KMHT(W)-600/600 /KMHT(W)-750/750 /KMHT(W)-900/900

 • Size: Bespoke /Manufacturer's standard

 • Loading: FACTA AAA /FACTA B /FACTA C /FACTA D

 • Material: 304L stainless steel /316L stainless steel

 • Accessories: None /Enclosed fire-rated insulated panel

Suggested Specification:

Kent Triple Seal Water Tight

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Triple Seal Water Tight Manhole

 • Type: KMHT(W)-600/600

 • Size: 600mm x 600mm clear opening

 • Loading: FACTA C

 • Material: 316L stainless steel

 • Accessories: Enclosed fire-rated insulated panel