NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKH215110)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKH215110)

Product Specification:

KV215/110V

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Industrial Gully – Side Outlet

• Type: KV215/110V /KV215/110VDS /KV315/110V /KV315/110VDS /KV315/160V /KV315/160VDS

• Height: Manufacturer's standard /Bespoke

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Loading class to BS EN 1253: L15 /R50 /M125 /N250 /P400

• Flange type: 4” 150lb R/F S/O ANSI Flange /4” PN10 R/F S/O Flange /Damp proof membrane flange /Holding flange /Puddle flange

• Side inlets:

- Type: 1½” BSP nipple /1½” BSP socket /50 mm push fit /Above ground funnel

- Angle: 45° /90° /Bespoke

• Grating:

• Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

• Accessories: None /Hinged self-sealing stainless bung

Suggested Specification:

KV215/110V

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Industrial Gully – Side Outlet

• Type: KV215/110VDS

• Height: Manufacturer's standard

• Material: 1.4301 (304) stainless steel

• Loading class to BS EN 1253: M125

• Flange type: None

• Side inlets: None

• Grating: KMG Kent Mesh Grating

• Filter basket: /Required

• Accessories: None