**Kent Bus RTPI Pole KBRTP 3000/3**

Kent Bus RTPI Pole KBRTP3000/3; 3000mm Overall Height; 3mm Wall Thickness; 101mm Diameter; Grade 316L Stainless Steel; Bright Satin Finish; Cast in. The Kent Bus RTPI poles offer a sturdy solution to the installation and mounting of RTPI (Real Time Passenger Information) display cases. The freestanding poles come in 3000mm lengths with a range of options available. An integrated lockable door is provided as standard as well as a cable entry point. These poles were designed to incorporate new RTPI displays for Dublin Bus. They are available in under-mount and side- mount variations.

**Features**

* Grade 316 stainless steel
* Cable entry point
* Heavy Duty Stainless steel pawl lock
* Integrated access door
* Vandal Resistant – minimum 3mm thick stainless steel throughout