NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/334 Stainless steel rodding eyes

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKRCR1804RoddingEye)

* [390 RODDING EYES](https://www.ribaproductselector.com/products/rodding-eyes/R11_390.aspx)

Product Specification:

KVV225RE Rodding Eye

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Rodding Eye

• Type: KVV225RETP /KVV225RE KVBO

• Loading class to BS EN 1253: L15 /R50 /M125 /N250 /P400

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Cover: Sealed cover

• Finish: Satin

Suggested Specification:

KVV225RE KVBO Rodding Eye

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Rodding Eye (Vinyl Floor)

• Type: KVV225RE KVBO

• Loading class to BS EN 1253:M125

• Material: 1.4401 (316) stainless steel

• Cover: Sealed cover