NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor channels

NBS Specification:



This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [315 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

 KSIC125 Shallow Invert Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Shallow Invert Channel

• Type: KSIC125 /KSIC150

• Length:

• Loading class to BS EN 1433: A15 /B125

• Material: 1.4301 (304) stainless steel /1.4404 (316L) stainless steel

• Grating:

• Accessories: None /Lockdown option /Trapped /Untrapped

Suggested Specification:

KSIC125 Shallow Invert Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Shallow Invert Channel

• Type: KSIC125

• Length: 1500mm

• Loading class to BS EN 1433: A15

• Material: 1.4404 (316L) stainless steel

• Grating: Kent Pedestrian Heelmesh (9mm)

• Accessories: Lockdown option / Untrapped