NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

* [340 CYCLE SHELTER](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

Product Specification:

Kent Dundrum Cycle Shelter

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Dundrum Cycle Shelter (KDS/7)

• Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

• Size :

* Width : 4000 mm /Special order
* Length: 5 Bay (10000mm) / 7 Bay (15000mm) / Special Order
* Height: 2600 mm /Special order

• Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened / Powder-coated, metallic black /Powder-coated, RAL /Other

• Glass: 20mm laminated

• Installation Type: Buried flange /Cast-in /Visible flange / 2 stage cast in

• Accessories/ Other requirements: /lighting/integrated cycle racks

Suggested Specification:

Kent Dundrum Cycle Shelter

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Dundrum Cycle Shelter (KDS/7)

• Material: Galvanized carbon steel

• Size :

* Width : 4000 mm
* Length: 5 Bay (10000mm)
* Height: 2600 mm

• Finish: Powder-coated, metallic black

• Glass: 20mm laminated

• Installation Type: 2 stage cast in

• Accessories/ Other requirements: integrated cycle racks