NBS Specification:



This product is associated with the following NBS Create clause:

25-25-10/110 Balustrade and guarding system

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[L30 Stairs/ ladders/ walkways/ handrails/ balustrades](https://www.ribaproductselector.com/products/stairs-ladders-walkways-handrails-balustrades/L30.aspx)

* [560 PROPRIETARY BALUSTRADES](https://www.ribaproductselector.com/products/proprietary-balustrades/L30_560.aspx)

Product Specification:

Kent Light Rail Balustrade Straight KLRB 1200(S)

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Light Rail Balustrade Straight KLRB 1200(S)

• Type: Surface Mounted

• Size:

* Height: 1200 mm /Special order
* Length: 1600 mm /Special order
* Width : 50 mm /Special order

• Finish: Bead blasted /Bright satin /Electropolished /Satin 320 grit polish