NBS Specification:



This product is associated with the following NBS Create clause:

NBS Specification:



This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

* [305 PROPRIETARY ACCESS AND INSPECTION CHAMBERS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

Product Specification:

Kent Bench Bottom Manhole Liner Square/ Round

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Benched Bottom Manhole Liner

 • Type: KBBML850 /KBBML1000 /KBBML1200RD /KBBML700-700SQ /KBBML950-950SQ /KBBML1200-1200SQ /Bespoke

 • Loading to BS EN 1433: B125 /C250 /D400

 • Body size:

 • Inlet:

 - Size:

 - Quantity: 1 /2 /3 /As drawing

 • Step rungs: Not required /Required

Suggested Specification:

Kent Bench Bottom Manhole Liner Square/ Round

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Benched Bottom Manhole Liner

 • Type: KBBML1200RD

 • Loading to BS EN 1433: B125

 • Body size: As per project requirement

 • Inlet: As per project requirement

 - Size: As per project requirement

 - Quantity: 1 /2 /3 /As drawing

 • Step rungs: Not required /Required