NBS Specification:



This product is associated with the following NBS Create clause:

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

* [305 PROPRIETARY ACCESS AND INSPECTION CHAMBERS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentBenchBottomManholeLinerSquareRound)

Product Specification:

Kent Bench Bottom Manhole Liner Square/ Round

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Benched Bottom Manhole Liner

• Type: KBBML850 /KBBML1000 /KBBML1200RD /KBBML700-700SQ /KBBML950-950SQ /KBBML1200-1200SQ /Bespoke

• Loading to BS EN 1433: B125 /C250 /D400

• Body size:

• Inlet:

- Size:

- Quantity: 1 /2 /3 /As drawing

• Step rungs: Not required /Required