NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

* [340 CYCLE SHELTER](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

Product Specification:

Kent Blanchardstown Cycle Shelter KBBS 4100

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 (0)53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Blanchardstown Cycle Shelter (KBBS/4100)

• Material: Galvanized carbon steel / Powdercoated to RAL

• Covering: 20mm toughened and laminated

• Size :

* Width : 2210mm
* Length: 2050mm / 4100mm / 6150mm
* Height: 2100mm

• Finish: Galvanised / Powdercoated

• Installation Type: Visible flange

• Accessories/ Other requirements: Integrated cycle rack

Suggested Specification:

Kent Blanchardstown Cycle Shelter KBBS 4100

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 (0)53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Blanchardstown Cycle Shelter (KBBS/4100)

• Material: Galvanized carbon steel / Powdercoated to RAL

• Covering: 20mm toughened and laminated

• Size :

* Width : 2210mm
* Length: 6150mm
* Height: 2100mm

• Finish: Powdercoated

• Installation Type: Visible flange

• Accessories/ Other requirements: Integrated cycle rack