NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:



This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

* [340 CYCLE SHELTER](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

Product Specification:

Kent Blanchardstown Cycle Shelter KBBS 4100

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +353 (0)53 914 3216

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Blanchardstown Cycle Shelter (KBBS/4100)

• Material: Galvanized carbon steel / Powdercoated to RAL

 • Covering: 20mm toughened and laminated

 • Size :

* Width : 2210mm
* Length: 2050mm / 4100mm / 6150mm
* Height: 2100mm

 • Finish: Galvanised / Powdercoated

 • Installation Type: Visible flange

 • Accessories/ Other requirements: Integrated cycle rack

Suggested Specification:

Kent Blanchardstown Cycle Shelter KBBS 4100

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +353 (0)53 914 3216

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Blanchardstown Cycle Shelter (KBBS/4100)

• Material: Galvanized carbon steel / Powdercoated to RAL

 • Covering: 20mm toughened and laminated

 • Size :

* Width : 2210mm
* Length: 6150mm
* Height: 2100mm

 • Finish: Powdercoated

 • Installation Type: Visible flange

 • Accessories/ Other requirements: Integrated cycle rack