NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKCRM600AccessCover)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKCRM600AccessCover)

Product Specification:

Kent Commercial Range Access Cover KCRM600/600

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Commercial Manhole

• Type: KCRM300/300/32 / /KCRM450/450/32 / KCRM600/450/32 / KCRM600/600/32 / KCRM750/600/32 / KCRM750/750/32

• Size: 300mm x 300mm clear opening / 450mm x 450mm clear opening / 600mm x 450mm clear opening / 600mm x 600mm clear opening / 750mm x 600mm clear opening / 750mm x 750mm clear opening

• Loading: BS EN 1253 Class K3, FACTA Load class A

• Accessories: 4 no. locking points / shallow profile

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

Suggested Specification:

Kent Commercial Range Access Cover KCRM600/600

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Commercial Manhole

• Type: KCRM600/600/32

• Size: 600mm x 600mm clear opening

• Loading: BS EN 1253 Class K3, FACTA Load class A

• Accessories: 4 no. locking points / shallow profile

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel