NBS Specification:



This product is associated with the following NBS Create clause:

45-05-75/315 Open sided shelters

NBS Specification:



This product is associated with the following NBS clauses:

[B91 Buildings in the landscape](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

* [340 CYCLE SHELTER](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureSheltersKentDundrumCycleShelter)

Product Specification:

Kent Dundrum Cycle Shelter

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Dundrum Cycle Shelter (KDS/7)

 • Material: 1.4307 (304L) stainless steel /1.4404 (316L) stainless steel /Galvanized carbon steel

• Size :

* Width : 4000 mm /Special order
* Length: 5 Bay (10000mm) / 7 Bay (15000mm) / Special Order
* Height: 2600 mm /Special order

 • Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened / Powder-coated, metallic black /Powder-coated, RAL /Other

 • Glass: 20mm laminated

 • Installation Type: Buried flange /Cast-in /Visible flange / 2 stage cast in

 • Accessories/ Other requirements: /lighting/integrated cycle racks

Suggested Specification:

Kent Dundrum Cycle Shelter

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Dundrum Cycle Shelter (KDS/7)

 • Material: Galvanized carbon steel

• Size :

* Width : 4000 mm
* Length: 5 Bay (10000mm)
* Height: 2600 mm

 • Finish: Powder-coated, metallic black

 • Glass: 20mm laminated

 • Installation Type: 2 stage cast in

 • Accessories/ Other requirements: integrated cycle racks