NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentMultiTrayInternalManholeKMHD1200600)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentMultiTrayInternalManholeKMHD1200600)

Product Specification:

Kent Multi Tray Internal Manhole (KMHD1200/600)

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Multi Tray Internal Manhole

• Type: KMHD-1200/600 / KMHD-1200/1200 / KMHD-1800/1200 / KMHD-1800/1800 / KMHD-2400/1200 / KMHD-2400/1800 / KMHD-2400/2400

• Loading: FACTA AAA /FACTA B /FACTA C /FACTA D

• Material: 304L stainless steel /316L stainless steel

• Accessories: None /Enclosed fire-rated insulated panel /Four lifting points modified to locking points

Suggested Specification:

Kent Multi Tray Internal Manhole (KMHD1200/600)

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Multi Tray Internal Manhole

• Type: KMHD-2400/1800

• Size: 2400mm x 1800mm clear opening

• Loading: FACTA D

• Material: 316L stainless steel

• Accessories: Four lifting points modified to locking points