NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:



This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentMultiTrayInternalManholeKMHD1200600)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentMultiTrayInternalManholeKMHD1200600)

Product Specification:

Kent Multi Tray Internal Manhole (KMHD1200/600)

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Multi Tray Internal Manhole

 • Type: KMHD-1200/600 / KMHD-1200/1200 / KMHD-1800/1200 / KMHD-1800/1800 / KMHD-2400/1200 / KMHD-2400/1800 / KMHD-2400/2400

 • Loading: FACTA AAA /FACTA B /FACTA C /FACTA D

 • Material: 304L stainless steel /316L stainless steel

 • Accessories: None /Enclosed fire-rated insulated panel /Four lifting points modified to locking points

Suggested Specification:

Kent Multi Tray Internal Manhole (KMHD1200/600)

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Multi Tray Internal Manhole

 • Type: KMHD-2400/1800

 • Size: 2400mm x 1800mm clear opening

 • Loading: FACTA D

 • Material: 316L stainless steel

 • Accessories: Four lifting points modified to locking points