NBS Specification:



This product is associated with the following NBS Create clause:

45-75-95/465 Wall protection panels

NBS Specification:



This product is associated with the following NBS clauses:

[N10 General fixtures/ furnishings/ equipment](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

* [350 MISCELLANEOUS FITTINGS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

[P20 Unframed isolated trims/ skirtings/ sundry items](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

 [170 PROPRIETARY](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Surface-ProtectionKentStainlessKerbing)

Product Specification:

Kent Stainless Double Sided Kerbing

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Stainless Double Sided Kerbing

 • Type: KDSK290 /KDSK630

 • Material:

 - Type: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

 - Thickness: 2 mm /3 mm

 - Finish: 320 grit polished and electropolished /Bead blasted /Bead blasted and electropolished /Electropolished /Satin, 320 grit polished /Powder coated

 • Fixing: Buried flange /Cast in /Flange /Hidden flange

 • Cowl: Required /Not required