NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:



This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/products/trenches-pipeways-and-pits-for-buried-engineering-services/P30.aspx)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-manhole-tops-and-frames/P30_301.aspx)

[P31 Holes, chases, covers and supports for services](https://www.ribaproductselector.com/products/holes-chases-covers-and-supports-for-services/P31.aspx)

* [370 ACCESS COVERS/ GRATINGS FOR](https://www.ribaproductselector.com/products/access-covers-gratings-for/P31_370.aspx)

[R12 Below ground drainage systems](https://www.ribaproductselector.com/products/below-ground-drainage-systems/R12.aspx)

* [471 ACCESS COVERS AND FRAMES](https://www.ribaproductselector.com/products/access-covers-and-frames/R12_471.aspx)

Product Specification:

Kent Vinyl Manhole KMHD-600/600V

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Internal Vinyl Manhole

 • Type: KHMD-300/300V / KMHD-450/450V / KMHD-600/600V / KMHD-750/750V / KMHD-900/900V

 • Size: Bespoke /Manufacturer's standard

 • Loading: FACTA AAA /FACTA B /FACTA C /FACTA D

 • Material: 304L stainless steel /316L stainless steel

 • Accessories: None /Enclosed fire-rated insulated panel /Open from underneath /Safety grid

Suggested Specification:

Kent Vinyl Manhole KMHD-600/600V

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Internal Vinyl Manhole

 • Type: KMHD-600/600V

 • Size: 600mm x 600mm clear opening

 • Loading: FACTA B

 • Material: 316L stainless steel

 • Accessories: None