NBS Specification:



This product is associated with the following NBS Create clause:

45-35-82/407 Signboards

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N91 External signage and interpretation](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureWayfindingKentLightRailNoticeBoard)

* [530 LOCKABLE NOTICEBOARD/ DISPLAY CABINET](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureWayfindingKentLightRailNoticeBoard)

Product Specification:

Kent Light Rail Notice Board

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Light Rail Notice Board (KLRNB1375) /Kent Light Rail Notice Board (KLRNB1375 DS)

• Type: Buried flange /Cast-in /Visible flange

• Material: Stainless steel, grade 304L (1.4304) /Stainless steel, grade 316L (1.4404)

• Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened