NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[N91 External signage and interpretation](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureWayfindingKentDohaFingerPost)

* [520 MONOLITH/ ENTRANCE/ WELCOME SIGN](https://www.ribaproductselector.com/products/monolith-entrance-welcome-sign/N91_520.aspx)

Product Specification:

Kent Light Rail RTPI Pole KLRTP 3000/3

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Light Rail RTPI Pole KLRTP 3000/3

• Size:

- Height: 3000mm

• Type: Buried flange /Cast-in /Visible flange

• Material: Stainless steel, grade 304L (1.4304) /Stainless steel, grade 316L (1.4404)

• Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened

• Printing/ Font:

• Finial: