NBS Specification:



This product is associated with the following NBS clauses:

[N91 External signage and interpretation](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Street-FurnitureWayfindingKentDohaFingerPost)

* [520 MONOLITH/ ENTRANCE/ WELCOME SIGN](https://www.ribaproductselector.com/products/monolith-entrance-welcome-sign/N91_520.aspx)

Product Specification:

Kent Wayfinding Lectern KWFL1207

 • Manufacturer: Kent Stainless

 Web: www.kentstainless.com

 Email: info@kentstainless.com

 Tel: +44 (0) 800 376 8377

 Fax: +353 53 914 1802

 Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

 • Product reference: Kent Wayfinding Lectern KWFL1207

 • Size:

 - Height: 1207mm

 - Width: 1000mm

 - Diameter: 100mm

 • Type: Buried flange /Cast-in /Visible flange

 • Material: Stainless steel, grade 304L (1.4304) /Stainless steel, grade 316L (1.4404)

 • Finish: Bright peened /Bright satin /Electropolished /Satin 320 grit polish /Shot peened