NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Access-CoversKentHingedMultiPaverKHMP)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=kentstainless-Access-CoversKentHingedMultiPaverKHMP)

Product Specification:

Kent Thames Water Access Cover KTWHLA-600

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Kent Thames Water Access Cover KTWHLA

• Type: KTWHLA600

• Size: 688mm x 688mm clear opening

• Load class: BS EN 124 C250

• Performance: Opening Effort <10kg

• Lifting Aid: Mechanical Compression Spring Struts

• Material: 1.4404 (316L)stainless steel

• Tray depth: 94mm (up to 80mm deep paving)

• Lettering (lifting corners): Required (Thames Water)

Options

• Seal: (double sealed) Required /Not required

• Safety barrier: Required /Not required

• Safety grid: Required /Not required