NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/302 Floor channels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [310 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

Superwide Slot Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Superwide Slot Channel

• Type: KSSC44/250/110 / KSSC44/250/160

• Material: Grade 1.4307 (304L) stainless steel /Grade 1.4404 (316L) stainless steel

• Loading: FACTA B / FACTA C / FACTA D // BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400

• Access cover: Recessed access box with centre fixed visible slots

• Outlet point: 300mm x 150mm x 100mm

Suggested Specification:

Superwide Slot Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Superwide Slot Channel

• Type: KSSC44/250/110

• Material: Grade(316L) stainless steel

• Loading: FACTA B

• Access cover: Recessed access box with centre fixed visible slots

• Outlet point: 300mm x 150mm x 100mm